|  |  |  |
| --- | --- | --- |
| Product: | 40-255/901G | 255.JPG |
| Article number: | Please contact our sales department. |
| Product Description: | 40mm child resistant closure with liner and tamper evidence band adapted for “40 potent UN-thread” (grov UN-gänga).  |
| **Technical specifications** |
| Drawings: | Product drawing: S 40-255\_901GNeck drawing: H 255 |
| Sealing: | Liner EPE/ALU |
| Plastic resin: | Cover: HDPEClosure: HDPE |
| Master batch: | Please contact our sales department. |
| Recommended capping torque: | 2,5–3,0 Nm |
| Storage durability: | 1 year, keep room temperatured in tightly sealed cardboard boxes.  |
| Certificate | ZE 06291531113-8317The package can only be designated as child resistant and suitable for adults if certified package are used according to ISO 8317. |
| **Quality Control** |
| Standards and norms | Sampling procedure: SS 020130-ISO2859 normal 1Defect classes according to KP-002  |
| **Delivery** |
| Packaging | 1.000 pcs packed in plastic bag, packed in cardboard boxes 82dm3. Labels on the boxes. 16 boxes on each pallet with stretch film wrapped around. |
| Traceability | Marking for traceability contains EVP article number, customer article number, production order number, pieces per carton, EVP order number customer order number and date and signature. |