|  |  |  |
| --- | --- | --- |
| Product: | 13-292 | G:\EVP info\Produktinformation - standardsortimentet\Kapsylbilder\Tubhatt\292-15 Rund.JPG |
| Article number: | Please contact our sales department. |
| Product Description: | 13mm tube closure with round piercing pin adapted for M13 thread.  |
| **Technical specifications** |
| Drawings: | Product drawing: S 13-291Neck drawing: M13 |
| Sealing: | - |
| Plastic resin: | PPH |
| Master batch: | Please contact our sales department. |
| Recommended Capping torque: | 0,1-0,3 Nm |
| Storage durability: | 1 year, keep room temperatured in tightly sealed cardboard boxes.  |
| **Quality Control** |
| Standards and norms | Sampling procedure: SS 020130-ISO2859 normal 1Defect classes according to KP-002  |
| **Delivery** |
| Packaging | 9000 pcs packed in plastic bag, packed in cardboard boxes 45dm3. Labels on the boxes. 24 boxes on each pallet with stretch film wrapped around.  |
| Traceability | Marking for traceability contains EVP article number, customer article number, production order number, pieces per carton, EVP order number customer order number and date and signature. |