|  |  |  |  |
| --- | --- | --- | --- |
| Product: | | 15-980 F | 980 fasett |
| Article number: | | Please contact our sales department. |
| Product Description: | | Tube closure with Facet adapted for M15-thread. |
| **Technical specifications** | | |
| Drawings: | | Product drawing: S 15-980F Neck drawing: H 15-980 | |
| Plastic resin: | | PPH | |
| Master batch: | | Please contact our sales department. | |
| Recommended Capping torque: | | 0,4-0,7 Nm | |
| Storage durability: | | 1 year, keep room temperatured in tightly sealed cardboard boxes. | |
| **Quality Control** | | | |
| Standards and norms | | Sampling procedure: SS 020130-ISO2859 normal 1  Defect classes according to KP-002 | |
| **Delivery** | | | |
| Packaging | 2000 pcs packed in plastic bag, packed in cardboard boxes 82dm3. Labels on the boxes. 16 boxes on each pallet with stretch film wrapped around. | | |
| Traceability | Marking for traceability contains EVP article number, customer article number, production order number, pieces per carton, EVP order number customer order number and date and signature. | | |